<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.32.3-Lima">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>GEOGCRS["Mexico ITRF2008",DATUM["Mexico ITRF2008",ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],CS[ellipsoidal,2],AXIS["geodetic latitude (Lat)",north,ORDER[1],ANGLEUNIT["degree",0.0174532925199433]],AXIS["geodetic longitude (Lon)",east,ORDER[2],ANGLEUNIT["degree",0.0174532925199433]],USAGE[SCOPE["Horizontal component of 3D system."],AREA["Mexico - onshore and offshore."],BBOX[12.1,-122.19,32.72,-84.64]],ID["EPSG",6365]]</wkt>
      <proj4>+proj=longlat +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +no_defs</proj4>
      <srsid>28806</srsid>
      <srid>6365</srid>
      <authid>EPSG:6365</authid>
      <description>Mexico ITRF2008</description>
      <projectionacronym>longlat</projectionacronym>
      <ellipsoidacronym>EPSG:7019</ellipsoidacronym>
      <geographicflag>true</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
